IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement[CatalogArticle]"
Time stamp: "2022-10-10T14:19:26"
Preprocessor: "IfcOpenShell 0.5.0-dev"
Originating system: "IfcOpenShell 0.5.0-dev"
Application: "CREATON CAD Bibliothek" version "0.5.0-dev" identifier "CREATON CAD Bibliothek" by Organization "cc" id "cc" description "cc"

People and organizations
  Person "cc" "cc" id "cc" of Organization "cc" id "cc" description "cc"
  Owner history of Person "cc" "cc" id "cc" of Organization "cc" id "cc" description "cc" | application "CREATON CAD Bibliothek" version "0.5.0-dev" identifier "CREATON CAD Bibliothek" by Organization "cc" id "cc" description "cc" | change ADDED | created 1665404366 (2022-10-10T12:19:26Z) | last modified 1665404366 (2022-10-10T12:19:26Z) by Person "cc" "cc" id "cc" of Organization "cc" id "cc" description "cc" with "CREATON CAD Bibliothek" version "0.5.0-dev" identifier "CREATON CAD Bibliothek" by Organization "cc" id "cc" description "cc"

Units
  LENGTHUNIT: MILLI METRE
  PLANEANGLEUNIT: Degrees (conversion based)

Spatial structure
IFCPROJECT
  IFCSITE
    IFCBUILDING
      IFCBUILDINGSTOREY
        contains 1 element
          1 x IFCDISCRETEACCESSORY | names: "Unknown name" | descriptions: "Unknown description" | property sets: Pset_ManufacturerTypeInformation

Property sets
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCDISCRETEACCESSORY)
    Bestellcode Farbe (konkateniert) = "845" (IFCTEXT)
    Bestellcode Farbe = "zinkgrau" (IFCTEXT)
    Bestellcode Farbe Name = "845" (IFCTEXT)
    Bestellcode Funktion = "Flächenstein" (IFCTEXT)
    Bestellcode Funktion Name = "1001" (IFCTEXT)
    Bestellcode Modell = "HEIDELBERG" (IFCTEXT)
    Bestellcode Modell Name = "801" (IFCTEXT)
    Dachneigung DUO extra (A) = "≥ 17 °" (IFCTEXT)
    Dachneigung DUO longlife ND extra (A) = "≥ 17 °" (IFCTEXT)
    Dachneigung QUATTRO longlife extra (A) = "≥ 15 °" (IFCTEXT)
    Dachneigung TRIO extra (A) = "≥ 17 °" (IFCTEXT)
    Deckbreite i.M. (ca.) = "300 mm" (IFCTEXT)
    Deckbreite max. (ca.) = "300 mm" (IFCTEXT)
    Deckbreite min. (ca.) = "300 mm" (IFCTEXT)
    Decklänge i.M. (ca.) = "328 mm" (IFCTEXT)
    Decklänge i.M. (ca.) AT = "325 mm" (IFCTEXT)
    Decklänge max. (ca.) = "345 mm" (IFCTEXT)
    Decklänge max. (ca.) AT = "340 mm" (IFCTEXT)
    Decklänge min. (ca.) = "310 mm" (IFCTEXT)
    Decklänge min. (ca.) AT = "310 mm" (IFCTEXT)
    Gewicht je Palette (ca.) = "1080 kg" (IFCTEXT)
    Gewicht je Palette (ca.) = "1110 kg" (IFCTEXT)
    Gewicht je Stück (ca.) = "4,5 kg/Stück" (IFCTEXT)
    Gewicht je m² (ca.) = "45,9 kg/m²" (IFCTEXT)
    Größe (ca.) - generiert = "334 x 420 x 61 mm" (IFCTEXT)
    Oberfläche = "planar" (IFCTEXT)
    Produktfamilie = "Profilierte Dachsteine" (IFCTEXT)
    Produktionswerk = "Neuburg" (IFCTEXT)
    Regeldachneigung CREATON AT in Kombination mit Zusatzmaßnahmen nach Herstellerangaben = "17 °" (IFCTEXT)
    Regeldachneigung CREATON CH in Kombination mit Zusatzmaßnahmen nach Herstellerangaben = "25 °" (IFCTEXT)
    Regeldachneigung CREATON DE in Kombination mit Zusatzmaßnahmen nach Herstellerangaben = "18 °" (IFCTEXT)
    UUID = "8d2f105c-febe-4a6e-a53e-033a4d26dac2" (IFCTEXT)
    Verpackung (generiert) = "240 Stk./Pal." (IFCTEXT)
    Ziegelbedarf i.M. (ca.) = "10,2 Stück/m²" (IFCTEXT)
    Ziegelbedarf max. (ca.) = "10,7 Stück/m²" (IFCTEXT)
    Ziegelbedarf min. (ca.) = "9,7 Stück/m²" (IFCTEXT)