IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement[CatalogArticle]"
Time stamp: "2022-09-30T14:11:33"
Preprocessor: "IfcOpenShell 0.5.0-dev"
Originating system: "IfcOpenShell 0.5.0-dev"
Application: "CREATON CAD Bibliothek" version "0.5.0-dev" identifier "CREATON CAD Bibliothek" by Organization "cc" id "cc" description "cc"

People and organizations
  Person "cc" "cc" id "cc" of Organization "cc" id "cc" description "cc"
  Owner history of Person "cc" "cc" id "cc" of Organization "cc" id "cc" description "cc" | application "CREATON CAD Bibliothek" version "0.5.0-dev" identifier "CREATON CAD Bibliothek" by Organization "cc" id "cc" description "cc" | change ADDED | created 1664539893 (2022-09-30T12:11:33Z) | last modified 1664539893 (2022-09-30T12:11:33Z) by Person "cc" "cc" id "cc" of Organization "cc" id "cc" description "cc" with "CREATON CAD Bibliothek" version "0.5.0-dev" identifier "CREATON CAD Bibliothek" by Organization "cc" id "cc" description "cc"

Units
  LENGTHUNIT: MILLI METRE
  PLANEANGLEUNIT: Degrees (conversion based)

Spatial structure
IFCPROJECT
  IFCSITE
    IFCBUILDING
      IFCBUILDINGSTOREY
        contains 1 element
          1 x IFCDISCRETEACCESSORY | names: "Unknown name" | descriptions: "Unknown description" | property sets: Pset_ManufacturerTypeInformation

Property sets
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCDISCRETEACCESSORY)
    Bestellcode Farbe (konkateniert) = "840" (IFCTEXT)
    Bestellcode Farbe = "klassikrot" (IFCTEXT)
    Bestellcode Farbe Name = "840" (IFCTEXT)
    Bestellcode Funktion = "Flächenstein" (IFCTEXT)
    Bestellcode Funktion Name = "1001" (IFCTEXT)
    Bestellcode Modell = "HEIDELBERG" (IFCTEXT)
    Bestellcode Modell Name = "801" (IFCTEXT)
    Gewicht je m² (ca.) = "45 kg/m²" (IFCTEXT)
    Gewicht je m² (ca.) = "45,9 kg/m²" (IFCTEXT)
    Größe (ca.) - generiert = "334 x 420 x 61 mm" (IFCTEXT)
    Produktfamilie = "Profilierte Dachsteine" (IFCTEXT)
    Regeldachneigung CREATON AT in Kombination mit Zusatzmaßnahmen nach Herstellerangaben = "17 °" (IFCTEXT)
    Regeldachneigung CREATON CH in Kombination mit Zusatzmaßnahmen nach Herstellerangaben = "25 °" (IFCTEXT)
    Regeldachneigung CREATON DE in Kombination mit Zusatzmaßnahmen nach Herstellerangaben = "18 °" (IFCTEXT)
    UUID = "3e0bd290-a092-4134-a771-4ef4d1337087" (IFCTEXT)